! common block definition file taken from respective MSC.Marc release and reformated to free format
!***********************************************************************
!
!        File: creeps.cmn
!
!        MSC.Marc include file
!
real(pReal)   cptim,timinc,timinc_p,timinc_s,timincm,timinc_a,timinc_b
integer(pInt) icfte,icfst,icfeq,icftm,icetem,mcreep,jcreep,icpa,icftmp,icfstr,&
              icfqcp,icfcpm,icrppr,icrcha,icpb,iicpmt,iicpa
real(pReal)   time_beg_lcase,time_beg_inc,fractol,time_beg_pst
!
integer(pInt) num_creepsr,num_creepsi,num_creeps2r
parameter(num_creepsr=7)
parameter(num_creepsi=17)
parameter(num_creeps2r=4)
common/marc_creeps/cptim,timinc,timinc_p,timinc_s,timincm,timinc_a,timinc_b,icfte,icfst,&
      icfeq,icftm,icetem,mcreep,jcreep,icpa,icftmp,icfstr,icfqcp,icfcpm,icrppr,icrcha,icpb,iicpmt,iicpa
common/marc_creeps2/time_beg_lcase,time_beg_inc,fractol,time_beg_pst
!
! cptim          Total time at begining of increment.
! timinc         Incremental time for this step.
! icfte          Local copy number of slopes of creep strain rate function
!                versus temperature. Is -1 if exponent law used.
! icfst          Local copy number of slopes of creep strain rate function
!                versus equivalent stress. Is -1 if exponent law used.
! icfeq          Local copy number of slopes of creep strain rate function
!                versus equivalent strain. Is -1 if exponent law used.
! icftm          Local copy number of slopes of creep strain rate function
!                versus time. Is -1 if exponent law used.
! icetem         Element number that needs to be checked for creep convergence
!                or, if negative, the number of elements that need to 
!                be checked. In the latter case the elements to check
!                are stored in ielcp.
! mcreep         Maximum nuber of iterations for explicit creep.
! jcreep         Counter of number of iterations for explicit creep 
!                procedure. jcreep must be .le. mcreep
! icpa           Pointer to constant in creep strain rate expression.
! icftmp         Pointer to temperature dependent creep strain rate data.
! icfstr         Pointer to equivalent stress dependent creep strain rate data.
! icfqcp         Pointer to equivalent creep strain dependent creep strain
!                rate data.
! icfcpm         Pointer to equivalent creep strain rate dependent
!                creep strain rate data.
! icrppr         Permanent copy of icreep
! icrcha         Control flag for creep convergence checking , if set to
!                1 then testing on absolute change in stress and creep
!                strain, not relative testing. Input data.
! icpb           Pointer to storage of material id cross reference numbers.
! iicpmt         
! iicpa          Pointer to constant in creep strain rate expression
!
!  time_beg_lcase  time at the beginning of the current load case
!  time_beg_inc    time at the beginning of the current increment
!  fractol         fraction of loadcase or increment time when we
!                  consider it to be finished
!  time_beg_pst    time corresponding to first increment to be
!                  read in from thermal post file for auto step
!
!***********************************************************************
!!$omp threadprivate(/marc_creeps/)
!!$omp threadprivate(/marc_creeps2/)
!! 
