{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["SDEP_EndSem"],"read":"whole","date_system":"1900"}

{"sheet":"SDEP_EndSem","index":0,"n_rows":50,"n_cols":20,"rows_kept":50}
["Source:","C:\\Users\\Phanindra\\Documents\\SDEP_EndSem\\SDEP_EndSem.kicad_sch"]
["Date:","4/16/2022 3:34:05 PM"]
["Tool:","Eeschema (5.99.0-13046-g4fe9f01eb0)"]
["Generator:","D:\\5.99\\bin\\scripting\\plugins/bom_csv_grouped_by_value.py"]
["Component Count:",21]
[]
["Individual Components:"]
[]
["Item","Qty","Reference(s)","Value","LibPart","Footprint","Datasheet","Category","DK_Datasheet_Link","DK_Detail_Page","Description","Digi-Key_PN","Family","MANUFACTURER","MAXIMUM_PACKAGE_HEIGHT","MPN","Manufacturer","PARTREV","STANDARD","Status"]
[null,null,"A1","MQ-7","MQ-7:MQ-7","MQ7:XDCR_MQ-7",{"$nulls":7},"Hanwei Electronics","10 mm",null,null,"N/A","Manufacturer Recommendations"]
[null,null,"BZ1","Buzzer","Device:Buzzer","Buzzer_Beeper:Buzzer_15x7.5RM7.6","~"]
[null,null,"C1","0.22u","Device:C","Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm","~"]
[null,null,"C2","0.22u","Device:C","Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm","~"]
[null,null,"C3","0.33u","Device:C","Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm","~"]
[null,null,"C4","0.33u","Device:C","Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm","~"]
[null,null,"D1","LED","Device:LED","LED_THT:LED_Rectangular_W3.0mm_H2.0mm","~"]
[null,null,"D2","LED","Device:LED","LED_THT:LED_Rectangular_W3.0mm_H2.0mm","~"]
[null,null,"J1","BOB-08891","BOB-08891:BOB-08891","BOB:SPARKFUN_BOB-08891",{"$nulls":7},"SPARKFUN"]
[null,null,"R1","10k","Device:R","Potentiometer_THT:Potentiometer_Alps_RK09L_Single_Vertical","~"]
[null,null,"R2","1k","Device:R","Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal","~"]
[null,null,"R3","1k","Device:R","Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal","~"]
[null,null,"R4","1k","Device:R","Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal","~"]
[null,null,"R5","2.2k","Device:R","Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal","~"]
[null,null,"R6","1k","Device:R","Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal","~"]
[null,null,"R7","1k","Device:R","Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal","~"]
[null,null,"RV1","10k","Device:R_Potentiometer","Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal","~"]
[null,null,"U1","TL431ILP","TL431ILP:TL431ILP","TL431:TO92127P520H660-3",{"$nulls":7},"Microsemi",{"$nulls":3},1.4,"IPC-7251"]
[null,null,"U2","ATMEGA328P-PU","ATMEGA328P-PU:ATMEGA328P-PU","Atmega:DIP794W46P254L2967H457Q28B",{"$nulls":7},"Atmel"]
[null,null,"U3","V7805-500","dk_DC-DC-Converters:V7805-500","digikey-footprints:3-SIP_Module_V7805-500","https://www.cui.com/product/resource/digikeypdf/v78-500.pdf","Power Supplies - Board Mount","https://www.cui.com/product/resource/digikeypdf/v78-500.pdf","/product-detail/en/cui-inc/V7805-500/102-1709-ND/1828602","DC DC CONVERTER 5V 2.5W","102-1709-ND","DC DC Converters",null,null,"V7805-500","CUI Inc.",null,null,"Active"]
[null,null,"Y1","Crystal","Device:Crystal","Oscillator:Oscillator_SMD_Abracon_ASCO-4Pin_1.6x1.2mm","~"]
[]
[]
[]
["Collated Components:"]
[]
["Item","Qty","Reference(s)","Value","LibPart","Footprint","Datasheet","Category","DK_Datasheet_Link","DK_Detail_Page","Description","Digi-Key_PN","Family","MANUFACTURER","MAXIMUM_PACKAGE_HEIGHT","MPN","Manufacturer","PARTREV","STANDARD","Status"]
[1,1,"A1","MQ-7","MQ-7:MQ-7","MQ7:XDCR_MQ-7",{"$nulls":7},"Hanwei Electronics","10 mm",null,null,"N/A","Manufacturer Recommendations"]
[2,1,"BZ1","Buzzer","Device:Buzzer","Buzzer_Beeper:Buzzer_15x7.5RM7.6","~"]
[3,2,"C1, C2","0.22u","Device:C","Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm","~"]
[4,2,"C3, C4","0.33u","Device:C","Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm","~"]
[5,2,"D1, D2","LED","Device:LED","LED_THT:LED_Rectangular_W3.0mm_H2.0mm","~"]
[6,1,"J1","BOB-08891","BOB-08891:BOB-08891","BOB:SPARKFUN_BOB-08891",{"$nulls":7},"SPARKFUN"]
[7,1,"R1","10k","Device:R","Potentiometer_THT:Potentiometer_Alps_RK09L_Single_Vertical","~"]
[8,5,"R2, R3, R4, R6, R7","1k","Device:R","Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal","~"]
[9,1,"R5","2.2k","Device:R","Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal","~"]
[10,1,"RV1","10k","Device:R_Potentiometer","Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal","~"]
[11,1,"U1","TL431ILP","TL431ILP:TL431ILP","TL431:TO92127P520H660-3",{"$nulls":7},"Microsemi",{"$nulls":3},1.4,"IPC-7251"]
[12,1,"U2","ATMEGA328P-PU","ATMEGA328P-PU:ATMEGA328P-PU","Atmega:DIP794W46P254L2967H457Q28B",{"$nulls":7},"Atmel"]
[13,1,"U3","V7805-500","dk_DC-DC-Converters:V7805-500","digikey-footprints:3-SIP_Module_V7805-500","https://www.cui.com/product/resource/digikeypdf/v78-500.pdf","Power Supplies - Board Mount","https://www.cui.com/product/resource/digikeypdf/v78-500.pdf","/product-detail/en/cui-inc/V7805-500/102-1709-ND/1828602","DC DC CONVERTER 5V 2.5W","102-1709-ND","DC DC Converters",null,null,"V7805-500","CUI Inc.",null,null,"Active"]
[14,1,"Y1","Crystal","Device:Crystal","Oscillator:Oscillator_SMD_Abracon_ASCO-4Pin_1.6x1.2mm","~"]